Mark Bollinger

5-20-2016

DWD420

Chapter 13 review questions

1. This is the simplest form of addressing in which the operand value is present in the instruction. This mode can be used to define and use constants or set initial values of variables.
2. A simple form of addressing in which the address field contains the effective address of the operand. The technique was common in earlier generations of computers but is not common on contemporary architectures.